# controlled-interface-type

#### Syntax

controlled-interface-type { controlledInterfaceType | set | superset }

no controlled-interface-type { controlledInterfaceType | all }

#### Release Information

Command introduced in JunosE Release 7.1.0.

set and superset keywords added in JunosE Release 9.2.0.

#### Description

Assigns controlled-interface types to a QoS parameter definition. Controlled-interface types specify the types of logical interfaces whose queues and nodes can be controlled by instances of the parameter definition. You can specify up to four controlled-interface types for each parameter definition. The no version removes the controlled-interface type from the parameter definition.

#### Options

- controlledInterfaceType—One of the following controlled-interface types: atm, atm-vc, atm-vp, bridge, ethernet, fr-vc, ip, ip-tunnel, ipv6, l2tp-session, l2tp-tunnel, lsp, serial, svlan, server-port, vlan
- set—Specifies an interface set as a controlled-interface type
- superset—Specifies an interface superset as a controlled-interface type
- all—Removes all controlled-interface types

#### Mode

QoS Parameter Definition

#### Related Documentation

- Configuring a Basic Parameter Definition for QoS Administrators
- Creating a QoS Parameter on an Interface Superset or Interface Set