Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Monitoring LDP-Related Settings for VPLS, Monitoring MPLS Forwarding for Layer 2 Services over MPLS, and Monitoring MPLS Forwarding State for L2VPN (VPWS) Instances in the JunosE BGP and MPLS Configuration Guide

# show mpls forwarding

#### Syntax

show mpls forwarding
[ interface interfaceType interfaceSpecifier ] [ bgp | ldp | rsvp-te ]
[ label { atm vpi vci | labelNumber [ labelRangeEnd ] } ]
[ brief | bindings | bindings delta | delta ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays the MPLS forwarding table.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- bgp—Displays BGP-specific forwarding information
- ldp—Displays LDP-specific forwarding information
- rsvp-te—Displays RSVP-TE–specific forwarding information
- atm—Displays information for the specified ATM VPI/VCI labels
  - vpi—Specifies ATM VPI that partially designates a label
  - vci—Specifies ATM VCI that partially designates a label
- labelNumber—Label number, in the range 16–1048575
- labelRangeEnd—Number, in the range 16–1048575, that specifies the high end of a range of labels
- brief—Displays only brief or summary information about the tunnels
- bindings—Displays protocol-specific label-to-FEC bindings
- detail—Displays detailed information
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- Monitoring LDP-Related Settings for VPLS, Monitoring MPLS Forwarding for Layer 2 Services over MPLS, and Monitoring MPLS Forwarding State for L2VPN (VPWS) Instances in the JunosE BGP and MPLS Configuration Guide

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out