# ip rpf-route

#### Syntax

ip rpf-route ipAddress addressMask
{ nextHopIpAddress | nextHopInterfaceType nextHopInterfaceSpecifier }
[ distanceValue ] [ tag tagValue ]

[ no ] ip rpf-route ipAddress addressMask

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Customizes static routes that the router can use to verify source addresses in multicast packets. The no version removes the static route.

#### Options

- ipAddress—IP address of the destination network
- addressMask—Subnet mask for the destination network
- nextHopIpAddress—IP address of the next hop
- nextHopInterfaceType—Interface type; see Interface Types and Specifiers
- nextHopInterfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- distanceValue—Number in the range 0–255 that indicates the preference for this route
- tagValue—Number in the range 0–4294967295 that identifies the route in the routing table

#### Mode

Global Configuration