# ip vrrp authentication-type

#### Syntax

ip vrrp vrid authentication-type { none | text }

no ip vrrp vrid authentication-type

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the VRRP authentication type. The no version restores the default value, none.

#### Options

- vrid—VRID identifier; a number in the range 1–255
- none—Disables authentication
- text—Specifies simple text password

#### Mode

Interface Configuration