# exception monitor interval

#### Syntax

exception monitor interval interval

no exception monitor interval

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the interval at which you want the router to check NVS for core dump files. The no version disables the core dump monitor.

#### Options

- interval—Number of minutes between NVS checks; in the range 1–1440

#### Mode

Global Configuration