# monitor vlan interface

#### Syntax

monitor vlan interface interfaceType interfaceSpecifier
[ interfaceType interfaceSpecifier ]* [ load-interval seconds ] [ display-time-of-day ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays bit rate and packet rate statistics over a specified time interval for one or more VLAN subinterfaces. There is no no version.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers
  - atm
  - fastEthernet
  - gigabitEthernet
  - lag
  - tenGigabitEthernet
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- seconds—Number of seconds in the range 5–30 that specifies the time interval at which the router calculates bit rates and packet rates for the specified VLAN; default value is 5 seconds
- display-time-of-day—Sets time at which the router calculates the bit rate and packet rate statistics for the current interval
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Privileged Exec, User Exec