Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# type

#### Syntax

To configure the RTR operation:

[ no ] type rtrType protocol ipIcmpEcho destination
[ source-ipaddr srcAddr | source interfaceType interfaceSpecifier ]

To specify the L2TP tunnel type:

type tunnelType

no type

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

From RTR Configuration mode, configures an RTR operation. The no version removes the configured type from the operation and resets all configuration for an RTR index.

| Note: You must configure the operation’s type before you can configure any other characteristics of the operation.

From Domain Map Configuration and Tunnel Group Tunnel Configuration modes, specifies the L2TP tunnel type (RADIUS attribute 64, Tunnel-Type).

#### Options

- rtrType—One of the following types of operation:
  - echo—Performs end-to-end operation only
  - pathEcho—Discovers a path to the destination and echoes each device on the path
- destination—IP address or an IP hostname or domain name
- srcAddr—Source IP address
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- tunnelType—L2TP tunnel type

#### Mode

Domain Map Configuration, RTR Configuration, Tunnel Group Tunnel Configuration

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out