Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring CLI-Based Mirroring

# ip mirror

#### Syntax

ip mirror mirrorInterfaceType mirrorInterfaceSpecifier
[ analyzerInterfaceType analyzerInterfaceSpecifier [ next-hop nextHop ] ]

no ip mirror mirrorInterfaceType mirrorInterfaceSpecifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the specified interface to mirror all IP ingress and egress traffic, and directs the mirrored traffic to an analyzer interface. The no version disables mirroring on the interface.

| Note: This command is deprecated and might be removed completely in a future release. The function provided by this command has been replaced by the updated packet mirroring feature and the ip policy command used with the secure-input and secure-output keywords.

#### Options

- mirrorInterfaceType—Interface type; see Interface Types and Specifiers
- mirrorInterfaceSpecifier—Particular interface that performs the interface mirroring function; see Interface Types and Specifiers
- analyzerInterfaceType—Interface type
- analyzerInterfaceSpecifier—Particular interface used as the analyzer interface; if omitted, the virtual router's default analyzer interface is used
- nextHop—Next-hop IP address to the remote analyzer host; required if the analyzer interface is a shared medium, such as Ethernet

#### Mode

Global Configuration

## Related Documentation

- Configuring CLI-Based Mirroring

#### Published: 2011-04-07

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out