# redundant-port force-failover

#### Syntax

redundant-port interfaceType interfaceSpecifier [ force-failover ]

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Specifies a member link of a LAG bundle to fail over when more than one active member link exists. There is no no version.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- force-failover—Forces the specified port to fail over

#### Mode

Global Configuration