Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# snmp-server interfaces rfc1213

#### Syntax

snmp-server interfaces rfc1213 [ maxIfIndex ] [ maxIfNumber ]

[ no ] snmp-server interfaces rfc1213

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies that the router bases numbering in the IfTable on RFC 1213. The no version restores the default value, which is to use RFC 1573 style numbering in interface tables.

| Caution: Reducing the value of the maxIfIndex, the maxIfNumber, or both, causes the router to automatically reboot to factory default settings.

The router does not reboot to factory defaults if you:

#### Options

- Increase the values of maxIfIndex and/or maxIfNumber.
- Issue a no version of the snmp-server interfaces rfc1213 command when the router is already set up for RFC 1573 style numbering.
- Enter the snmp-server interfaces rfc1213 command with the same options multiple times.
- maxIfIndex—Maximum value of index numbers in the interface tables, in the range 100–65535; default value is 65535
- maxIfNumber—Maximum number of interfaces in each interface table, in the range 100–65535; default value is 65535

#### Mode

Global Configuration

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out