# address receive version

#### Syntax

address { ipAddress | unnumbered interfaceType interfaceSpecifier }
receive version { 1 | 2 | 1 2 | 2 1 | off }

no address [ ipAddress | unnumbered interfaceType interfaceSpecifier ] receive version

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Restricts the RIP version that the router can receive on an interface. The no version sets the interface back to the default value, receiving both RIP version 1 and version 2.

#### Options

- ipAddress—Address of IP interface where RIP will be run
- unnumbered—Specifies that RIP will be run on an unnumbered interface
  - interfaceType—Interface type; see Interface Types and Specifiers
  - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- 1—Specifies RIP version 1 only
- 2—Specifies RIP version 2 only
- 1 2—Specifies RIP version 1 and version 2; the default value
- 2 1—Specifies RIP version 2 and version 1
- off—Turns reception off

#### Mode

Address Family Configuration, Router Configuration