# ip rsvp bfd-liveness-detection

#### Syntax

{ ip | mpls } rsvp bfd-liveness-detection [ minimum-interval minInterval |
[ minimum-receive-interval minRecInterval ]
[ minimum-transmit-interval minTransInterval ] ] [ multiplier multValue ]

no { ip | mpls } rsvp bfd-liveness-detection

#### Release Information

Command introduced in JunosE Release 8.1.0.

#### Description

Enables BFD (bidirectional forwarding detection) on an interface running RSVP-TE and defines BFD values to be negotiated between RSVP-TE neighbors for detection of IP data path failures. See the mpls rsvp bfd-liveness-detection command for a complete description and syntax.

#### Mode

Interface Configuration