# l2tp switch-profile

#### Syntax

[ no ] l2tp switch-profile profileName

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Creates and names an L2TP tunnel switch profile. This command accesses L2TP Tunnel Switch Profile Configuration mode, from which you can define the L2TP tunnel switching behavior for the interfaces to which this profile is assigned. The no version removes the named tunnel switch profile from the router.

#### Options

- profileName—Name of the tunnel switch profile; a string of up to 64 alphanumeric characters

#### Mode

Global Configuration