Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring a Parameter Definition for IP Multicast Bandwidth Adjustment

# Guidelines for Configuring IP Multicast Adjustment for QoS

When you specify the IP multicast bandwidth adjustment application, the following considerations apply:

- You must specify a controlled-interface type.
- You cannot specify any instance-interface types or subscriber-interface types. By default, the system assigns a default instance-interface type of ip.
- When you specify the IP multicast bandwidth adjustment application, the parameter definition is hierarchical. You must specify the hierarchical keyword with the application keyword.
- The system prevents you from defining more than one parameter definition with the ip-multicast application specified. For example:
  host1(config)#qos-parameter-define vpShaper application ip-multicast hierarchical host1(config-qos-parameter-define)#controlled-interface-type ip host1(config-qos-parameter-define)#exit host1(config)#qos-parameter-define bar application ip-multicast hierarchical % there cannot be more than one parameter defined with this property
- Parameter instances associated with the IP multicast bandwidth adjustment application are not stored in non-volatile storage (NVS). (Parameter definitions are stored in NVS.) Because the application is activated based on IGMP joins and leaves received on an interface, the system removes the instances when you turn off or reset the router, then re-creates it based on new messages received on an interface.

## Related Documentation

- Configuring a Parameter Definition for IP Multicast Bandwidth Adjustment

#### Published: 2011-03-17

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out