# sscc protocol lac

#### Syntax

[ no ] sscc protocol lac

#### Release Information

Command introduced in JunosE Release 11.0.0.

#### Description

Configures the SRC client to support policy and QoS configuration on L2TP interfaces on a virtual router that functions as an L2TP access concentrator (LAC) on one side of an L2TP tunnel. The no version disables SRC client support for L2TP LAC interfaces.

| Note: You must enable the SRC client by using the sscc enable cops-pr command on the virtual router to be able to configure policy and QoS support for L2TP LAC interfaces by the COPS messages.

#### Mode

Global Configuration