# debounce

#### Syntax

debounce [ seconds ]

no debounce

#### Release Information

Command introduced in JunosE Release 9.3.0.

#### Description

Enables the debounce timer and sets the time interval that the interface waits before reporting a state change to the upper-layer protocols. The no version restores the default behavior, disabling debounce on the interface.

#### Options

- seconds—Interval for which an interface must maintain a given state before the interface reports the state change to the upper-layer protocols. Number in the range 1–5 seconds; default value is 1 second.

#### Mode

Interface Configuration