# radius override calling-station-id remote-circuit-id

#### Syntax

radius override calling-station-id remote-circuit-id

no radius override calling-station-id

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures RADIUS to override the standard use of the Calling-Station-Id [31] RADIUS attribute and instead use the PPPoE remote circuit ID transmitted from a DSLAM device. The no version restores the default Calling-Station-Id value, which is the telephone number from which the call originated.

#### Mode

Global Configuration