Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# rename

#### Syntax

rename [ sourcePath]sourceFilename [ destinationPath]destinationFilename

#### Release Information

Command introduced before JunosE Release 7.1.0.
hostName and deviceName variables added in JunosE Release 7.2.0.

#### Description

Renames a local file. There is no no version.

| Note: You cannot change the extension of a file, for example, from .mac to .scr. See Renaming Files in the JunosE System Basics Configuration Guide for detailed information on file type usage with the rename command.

#### Options

- sourcePath—Path to the source in the format:
  hostName: | deviceName: | /incoming/subdirectory/ | /outgoing/subdirectory/
  - hostName:—Name of the network host
  - deviceName:—Name of the device specifying a flash card slot
  - disk0—Specifies flash card slot 0 on the primary SRP module; if no device is specified for the primary SRP module, then disk0 is used
  - disk1—Specifies flash card slot 1 on the primary SRP module; source and destination file types must be .dmp; supported only on the E120 router and the E320 router
  - standby—Specifies flash card slot 0 on the standby SRP module for backward compatibility
  - standby-disk0—Specifies flash card slot 0 on the standby SRP module
  - standby-disk1—Specifies flash card slot 1 on the standby SRP module; source and destination file types must be .dmp; supported only on E120 and E320 routers
  - incoming—Specifies the router’s incoming FTP directory
  - subdirectory—Name of a subdirectory on the router’s FTP server. If the subdirectory does not exist, the router creates it.
  - outgoing—Specifies the router’s outgoing FTP directory
- sourceFileName—File to rename
- destinationPath—Path to the destination in the format:
  networkPath | /incoming/subdirectory | /outgoing/subdirectory
  - networkPath—Path to the network host
  - incoming—Specifies the incoming router’s FTP directory
  - subdirectory—Name of a subdirectory on the router’s FTP server. If the subdirectory does not exist, the router creates it.
  - outgoing—Specifies the router’s outgoing FTP directory
- destinationFileName—New filename

#### Mode

Privileged Exec

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out