Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring the Scheduler Hierarchy for Hashed Load Balancing in 802.3ad Link Aggregation Groups
- Configuring the Scheduler Hierarchy for Subscriber Load Balancing in 802.3ad Link Aggregation Groups
- Creating Parameter Instances
- For more information about other fields displayed with this command, see the JunosE Physical Layer Configuration Guide
- show interfaces lag members

# Monitoring the QoS Configuration of IEEE 802.3ad Link Aggregation Group Bundles

#### Purpose

Display information about the QoS configuration for Ethernet member links in all IEEE 802.3ad link aggregation group (LAG) bundles configured on the router, or about the member links in a specified IEEE 802.3ad LAG bundle.

#### Action

To display the QoS configuration for a specific LAG bundle:

    host1#show interfaces lag lg0 members
    Lag lg0 is Up, Administrative status is Up
    MAC Address is 0090.1a40.01be
    MTU: Operational 1526
    Duplex Mode: Operational Full Duplex
    Speed: Operational 100 Mbps
    System Priority 32768 System MAC Address is 0090.1a00.00e0 key 8
    Partner System Priority 0 System MAC Address is 0000.0000.0000 key 0
    QoS parameter: vlan 1500000
    Attached QoS profile: eth1
    Member-interface FastEthernet11/2 is Up
    (LACP disabled, state collecting/distributing)
    Member-interface FastEthernet11/3 is Down
    (LACP disabled, state waiting)
    Member-interface FastEthernet11/4 is Up
    (LACP disabled, state collecting/distributing)

#### Meaning

Table 1 lists the related show interfaces lag memberscommand output fields.

Table 1: show interfaces lag members Output Fields

Field Name | Field Description
--- | ---
Lag | Name of the LAG bundle
QoS parameter | QoS parameter instance at the displayed interface
Attached QoS profile | QoS profile attachment at the displayed interface

## Related Documentation

- Configuring the Scheduler Hierarchy for Hashed Load Balancing in 802.3ad Link Aggregation Groups
- Configuring the Scheduler Hierarchy for Subscriber Load Balancing in 802.3ad Link Aggregation Groups
- Creating Parameter Instances
- For more information about other fields displayed with this command, see the JunosE Physical Layer Configuration Guide
- show interfaces lag members

#### Published: 2011-03-21

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out