# timeout

#### Syntax

RADIUS:

timeout waitTime

no timeout

RTR:

timeout timeoutValue

no timeout

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

When used from RADIUS Configuration mode, specifies the interval, in seconds, before the router retransmits a RADIUS packet to an authentication or accounting server. The no version restores the default.

When used from RTR Configuration mode, specifies the timeout for a Response Time Reporter operation. The no version returns the operation to the default value. You can apply this parameter only to echo entries.

#### Options

- waitTime—Number of seconds in the range 1–1000; default value is 3
- timeoutValue—Number in milliseconds that the operation waits for a response; if the value is set to 0 or is larger than frequency, it will be ignored; default value is 5000

#### Mode

RADIUS Configuration, RTR Configuration