# baseline mpls label

#### Syntax

baseline mpls label { interface interfaceName atm vpi vci | labelValue }

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Sets a statistics baseline for the specified MPLS in label. Statistics for an in label must be enabled with the mpls statistics label command before they can be baselined. By default, the in-label counters are baselined at zero. There is no no version.

#### Options

- interfaceName—Name of interface for label in interface label space on an ATM AAL5 interface; up to 15 alphanumeric characters
- vpi—Virtual path identifier for a label, a value in the range 0–255
- vci—Virtual circuit identifier for a label, a value in the range 33–65535
- labelValue—Integer identifying a label in the platform label space, a value in the range 16–1048575

#### Mode

Privileged Exec