# ip igmp query-max-response-time

#### Syntax

ip igmp query-max-response-time tenthsOfaSecond

no ip igmp query-max-response-time

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the period in tenths of a second during which the host is expected to respond to an IGMP query. IGMP version 2 includes this value in IGMP query messages sent out on the interface. You cannot set this value on interfaces running IGMP version 1. The no version restores the default value, 100 tenths of a second (10 seconds).

#### Options

- tenthsOfaSecond—Time interval between receipt of an IGMP query and the response; in the range 1–254 tenths of a second.

#### Mode

Interface Configuration, Profile Configuration