# atm oam loopback-location

#### Syntax

atm oam loopback-location locationID

[ no ] atm oam loopback-location

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the location ID of the ATM interface. The no version returns the loopback location to the default setting of all 1s (ones).

#### Options

- locationID—Value of the four-octet long location ID of the ATM interface

#### Mode

Interface Configuration