# show ip bgp aggregate-address

#### Syntax

show ip bgp [ ipv4 unicast | ipv4 multicast | vpnv4 all | vpnv4 vrf vrfName ]
aggregate-address [ ipAddress mask ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays information about aggregate addresses.

#### Options

- ipv4 unicast—Specifies the IPv4 unicast address family and routing table; the default option
- ipv4 multicast—Specifies the IPv4 multicast address family and routing table
- vpnv4 all—Specifies the IPv4 VPN address family and all IPv4 VPN routing and forwarding instances
- vpvn4 vrf vrfName—Specifies the IPv4 VPN address family and only the IPv4 VPN routing and forwarding instance with the name vrfName
- ipAddress—Aggregate address
- mask—Aggregate address mask
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec