Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# radius ignore

#### Syntax

radius ignore attributeName { enable | disable }

no radius ignore attributeName

#### Release Information

Command introduced before JunosE Release 7.1.0.

pppoe-max-session keyword added in JunosE Release 9.3.0.

#### Description

Ignores the specified attribute in RADIUS Access-Accept messages. All attributes are disabled by default except for Framed-Ip-Netmask and Max-Clients-Per-Interface (pppoe-max-session). The no version restores the default.

#### Options

- attributeName—One of the following RADIUS attributes:
  - atm-mbs—Mbs, VSA 26-17
  - atm-pcr—Pcr, VSA 26-15
  - atm-scr—Scr, VSA 26-16
  - atm-service-category—Service-Category, VSA 26-14
  - egress-policy-name—Egress-Policy-Name, VSA 26-11
  - framed-ip-netmask—Framed-Ip-Netmask, attribute 9
  - pppoe-max-session—Max-Clients-Per-Interface, VSA 26-143
  - ingress-policy-name—Ingress-Policy-Name, VSA 26-10
  - virtual-router—Virtual-Router, VSA 26-1
- enable—Specifies the feature; this is the default setting for framed-ip-netmask and pppoe-max-session
- disable—Disables the feature; this is the default setting for all attributes except framed-ip-netmask and pppoe-max-session

#### Mode

Global Configuration

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out