# Monitoring the Redundancy Switchover History

#### Purpose

Display information about stateful SRP switchover history for the chassis.

#### Action

    host1# show redundancy switchover-history
                                                 system
    SRP activation time      type       slot     uptime          running release
    -------------------   -----------   ----   ----------   -------------------------
    2004-07-26 10:44:25   cold-start     07       ---       L-07-25-60b1mrg-e.rel
    2004-07-25 20:58:57   warm-switch    06    0 00:15:08   L-07-25-60b1mrg-e.rel
    2004-07-25 20:53:41   warm-switch    07    0 00:09:51   L-07-25-60b1mrg-e.rel
    2004-07-25 20:44:43   cold-start     06       ---       L-07-25-60b1mrg-e.rel
    2004-07-25 19:32:01   cold-start     06       ---       L-07-25-60b1mrg-d.rel
    2004-07-25 18:58:01   warm-switch    06    0 00:12:01   L-07-25-60b1mrg-c.rel
    2004-07-25 18:51:56   cold-switch    07    0 00:05:56   L-07-25-60b1mrg-c.rel
    2004-07-25 18:46:54   cold-start     06       ---       L-07-25-60b1mrg-c.rel
    2004-07-25 17:44:48   warm-switch    06    0 00:14:32   L-07-25-60b1mrg-b.rel
    2004-07-25 17:31:07   cold-start     07       ---       L-07-25-60b1mrg-b.rel
    2004-07-25 16:05:08   cold-start     07       ---       L-07-25-60b1mrg-a.rel
    2004-07-24 23:25:09   warm-switch    07    0 16:27:03   L-07-24-60b1mrg-b.rel
    2004-07-24 23:18:23   cold-switch    06    0 16:20:17   L-07-24-60b1mrg-b.rel

#### Meaning

Table 14 lists the show redundancy switchover-history command output fields.

Table 14: show redundancy switchover-history Output Fields

Field Name | Field Description
--- | ---
SRP activation time | Amount of time the SRP module has been active.
type | Type of switchover.
slot | Slot in which the SRP module resides.
system uptime | Amount of time the chassis has been operational.
running release | Release running on the SRP module at the time of the switchover.

#### Related Documentation

- show redundancy switchover-history