# isis priority

#### Syntax

isis priority value [ level-1 | level-2 ]

no isis priority [ level-1 | level-2 ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the priority of this router for designated router election. The no version resets priority to the default value, 64.

#### Options

- value—Number in the range 0–127; the priority of a router; default value is 64
- level-1—Sets the priority of a router for level 1 independently
- level-2—Sets priority of a router for level 2 independently

#### Mode

Interface Configuration, Subinterface Configuration