Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Monitoring VPLS-Specific Settings in the JunosE BGP and MPLS Configuration Guide

# show vpls connections

#### Syntax

show vpls connections [ state up | state down | details | bridge-group vplsName |
remote-site siteId ]* [ filter ]

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Displays connection information for a specified VPLS instance configured on the router, or for all VPLS instances configured on the router. You can display detailed configuration and status information for one or for all VPLS connections on the router, or you can display information only for VPLS connections with a specified operational state (up or down) or remote site ID.

#### Options

- state up—Displays information only for operational (up) VPLS connections
- state down—Displays information only for nonoperational (down) VPLS connections
- details—Displays detailed configuration and status information for VPLS connections
- vplsName—Name of a specific VPLS instance created with the bridge vpls transport-virtual-router command; if you omit the bridge-group keyword and VPLS instance name, the command displays connection information for all VPLS instances configured on the router
- siteId—Integer, in the range 1–65535, that uniquely identifies the remote site for a VPLS instance; the site ID is configured with the bridge vpls site-name site-id command
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- filter—See Filtering show Commands

#### Mode

Privileged Exec

## Related Documentation

- Monitoring VPLS-Specific Settings in the JunosE BGP and MPLS Configuration Guide

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out