# ip route-map ip-subscriber

#### Syntax

ip route-map ip-subscriber routeMapName

no ip route-map ip-subscriber

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures an interface for route-map processing and specifies the route map that is applied to the IP interface subscriber. If no route map is specified, then all packets will trigger the creation of a dynamic subscriber interface. The no version deletes the route map.

#### Options

- routeMapName—Name of route map

#### Mode

Interface Configuration, Profile Configuration