# framing

#### Syntax

framing framingType

no framing

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the framing mode used by E3 or T3 interfaces. Available modes vary by the type of interface. The no version restores the default for that interface.

#### Options

- framingType—One of the following framing types:

  E3 Frame

  - g751—Default; G.751 compliant frame
  - g832—G.832 compliant frame

  T3

  - c-bit—Default; specifies c-bit parity framing
  - m23—Specifies M23 multiplexer framing

#### Mode

Controller Configuration