# Monitoring Configured and Operational Status of All Tunnels

#### Purpose

Display a summary of the configured and operational status of all L2TP tunnels.

#### Action

To display a summary of the configured and operational status of all L2TP tunnels:

    host1#show l2tp tunnel summary

    Administrative status   enabled   drain   disabled
                            5         0       0
    Operational status      up        down    lower-down   not-present
                  5         0         0       0            0

#### Meaning

Table 95 lists the show l2tp tunnel summary command output fields.

Table 95: show l2tp tunnel summary Output Fields

Field Name | Field Description
--- | ---
Administrative status | Administrative status of all tunnels: enabled—No restrictions on the creation and operation of sessions for this tunnel drain—Router will not create new sessions for this tunnel disabled—Router disabled existing sessions and will not create new sessions for this tunnel
Operational status | Operational status of all tunnels: up—Tunnel is available down—Tunnel is unavailable lower-down—Tunnel is unavailable because the destination supporting it is inaccessible not-present—Tunnel is unavailable because the hardware (such as a line module) supporting the tunnel is inaccessible

#### Related Documentation

- show l2tp tunnel summary