Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# set extcommunity

#### Syntax

set extcommunity
{ rt extCommValue [ extCommValue ]* [ additive ] } | { soo extCommValue }

no set extcommunity

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the BGP extended communities attribute. The no version removes the set clause from a route map.

#### Options

- rt—Specifies a route-target extended community, which consists of one or more routers that can receive a set of routes advertised by BGP that carry the extended-community attribute
- soo—Specifies a site-of-origin extended community, which consists of one or more routers that inject into BGP a set of routes that carry the extended-community attribute
- extCommValue—Number identifying the extended community in one of the following formats:
  - AS:nn—Autonomous system number, in the range 1–65535, followed by an integer in the range 1–4294967295; for example, 320:72358
  - AS:nn—Autonomous system number, in the range 1–4294967295 followed by an integer in the range 1–65535; for example, 84511:45
  - ipAddress:nn—Dotted decimal IP address followed by an integer in the range 1–65535; for example, 10.10.21.5:1256
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- additive—Adds the specified extended communities to any previously configured for the attribute; if omitted, the specified extended communities replace any previously configured for the attribute

#### Mode

Route Map Configuration

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out