# ipv6 ospf priority

#### Syntax

ipv6 ospf [ processId ] priority intfPriority

no ipv6 ospf [ processId ] priority

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the router priority. Used in determining the designated router for the particular network. This designation applies only to multiaccess networks. Every broadcast and nonbroadcast multiaccess network has a designated router. The no version restores the default value.

#### Options

- processId—Integer in the range 1–65535
- intfPriority—Priority value, an 8-bit number in the range 1–255; default value is 1

#### Mode

Interface Configuration, Subinterface Configuration