# Monitoring QoS Configurations for L2TP

To monitor QoS configurations for L2TP:

- Monitoring the QoS Configuration of Fast Ethernet, Gigabit Ethernet, and 10-Gigabit Ethernet Interfaces
- Monitoring the QoS Configuration of IEEE 802.3ad Link Aggregation Group Bundles
- Monitoring the QoS Configuration of IP Interfaces
- Monitoring the QoS Profiles Attached to an Interface
- Monitoring the Configuration of QoS Port-Type Profiles
- Monitoring the Configuration of QoS Profiles
- Monitoring the QoS Scheduler Hierarchy
- Monitoring Shared Shapers