Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring Traffic Classes That Define Service Levels
- Configuring Traffic-Class Groups That Define Service Levels
- Policy Rule Precedence

# traffic-class

#### Syntax

In Classifier Group Configuration mode:

[ no ] [ suspend ] traffic-class trafficClassName1

In Global Configuration and Traffic Class Group Configuration modes:

[ no ] traffic-class trafficClassName2

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

In Classifier Group Configuration mode, specifies a traffic class in a policy list for policy management. The no version removes a traffic class from a policy list; the suspend version temporarily suspends the policy rule; the no suspend version resumes application of a suspended rule.

| Note: This command replaces the Policy List Configuration version of the traffic-class command, which may be removed completely in a future release.

In Global Configuration mode, configures a traffic class in the E Series router. In Traffic Class Group Configuration mode, specifies a traffic class that belongs to the traffic-class group. The no version deletes the traffic class.

#### Options

- trafficClassName1—Name of the traffic class; up to 40 characters
- trafficClassName2—Name of the traffic class; up to 31 characters

#### Mode

Classifier Group Configuration, Global Configuration, Traffic Class Group Configuration

## Related Documentation

- Configuring Traffic Classes That Define Service Levels
- Configuring Traffic-Class Groups That Define Service Levels
- Policy Rule Precedence

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out