# dsr-detect

#### Syntax

[ no ] dsr-detect

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Requires that a DSR signal be detected on the line for a user to log into the console. DSR is carried on pin 6 of the SRP module's RS-232 (DB-9) connector. The DSR input must be connected to the DSR output of a modem or the DTR output of another DTE device, such as a terminal server, that supports this signal. If a session is in progress and the DSR signal is lost, the user is logged out automatically. The no version restores the default of no DSR required.

#### Mode

Privileged Exec