# show mpls forwarding

#### Syntax

show mpls forwarding
[ interface interfaceType interfaceSpecifier ] [ bgp | ldp | rsvp-te ]
[ label { atm vpi vci | labelNumber [ labelRangeEnd ] } ]
[ brief | bindings | bindings delta | delta ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays the MPLS forwarding table.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- bgp—Displays BGP-specific forwarding information
- ldp—Displays LDP-specific forwarding information
- rsvp-te—Displays RSVP-TE–specific forwarding information
- atm—Displays information for the specified ATM VPI/VCI labels
  - vpi—Specifies ATM VPI that partially designates a label
  - vci—Specifies ATM VCI that partially designates a label
- labelNumber—Label number, in the range 16–1048575
- labelRangeEnd—Number, in the range 16–1048575, that specifies the high end of a range of labels
- brief—Displays only brief or summary information about the tunnels
- bindings—Displays protocol-specific label-to-FEC bindings
- detail—Displays detailed information
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Documentation

- Monitoring LDP-Related Settings for VPLS, Monitoring MPLS Forwarding for Layer 2 Services over MPLS, and Monitoring MPLS Forwarding State for L2VPN (VPWS) Instances in the JunosE BGP and MPLS Configuration Guide