# ethernet oam lfm pdu-lost-threshold

#### Syntax

[ no ] ethernet oam lfm pdu-lost-threshold pduLostPackets

#### Release Information

Command introduced in JunosE Release 11.1.0.

#### Description

Configures the number of OAM protocol data units (PDUs) that a local OAM client can fail to receive from a remote peer before a link-fault event is triggered. The no version removes the configured threshold for PDUs that can be missed from a remote peer before the generation of a link-fault event.

#### Options

- pduLostPackets—Number of expected OAM packets from the remote peer that the local OAM client can miss before a link-fault event is triggered; a number in the range 3–10; default value is 5

#### Mode

Interface Configuration

#### Related Documentation

- OAM Discovery Feature
- Configuring 802.3ah OAM Link-Fault Management
- ethernet oam lfm mode