Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# show l2tp tunnel

#### Syntax

show l2tp tunnel [ detail ] [ state { adminState | ifOperStatus |
failover-resync failoverResyncMode } ]
[ l2tpName | [ virtual-router vrName ] ip ipAddress [ l2tpNameNoDest ] ] [ filter ]

To display summary information:

show l2tp tunnel summary [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
failover-resync keyword and failoverResyncMode variable added in JunosE Release 9.0.0.

#### Description

Displays detailed information about the configured and operational status of selected L2TP tunnels or summary information for all L2TP tunnels.

#### Options

- detail—Provides complete information about the specified sessions, including the L2TP host profile name
- adminState—Displays information about tunnels only with the specified effective administrative state
  - enabled—Effective administrative state is disabled
  - disabled—Effective administrative state is enabled
  - drain—Effective administrative state is drain
- ifOperStatus—Displays information about tunnels only with the specified operational state
  - up—Operational state is up
  - down—Operational state is down
  - lower-down— Operational state is lower down
  - not-present—Operational state is not-present
- failoverResyncMode—Displays information about tunnels that use the specified failover resynchronization mode:
  - disable—Peer failover resynchronization is disabled
  - failover-protocol—Uses the L2TP failover protocol method
  - failover-protocol-fallback-to-silent-failover—Uses the L2TP failover protocol method; however, if the peer does not support this method, the silent failover method is used
  - not-configured—Uses the global failover method because peer failover resynchronization is not configured for L2TP host profiles and AAA domain map tunnels
  - silent-failover—Uses the L2TP silent failover method
- l2tpName—Tunnel name
- vrName—Name of the virtual router on which the tunnel exists
- ipAddress—IP address
- l2tpNameNoDest—Tunnel name
- filter—See Filtering show Commands
- summary—Displays the configured and operational status of all L2TP tunnels

#### Mode

Privileged Exec

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out