# clns configuration-time

#### Syntax

clns configuration-time configTime

no clns configuration-time

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the rate at which ES hellos and IS hellos are sent. The no version restores the default value, 10 seconds.

#### Options

- configTime—Number in the range 1–65535; rate in seconds at which ES and IS hello packets are sent; default value is 10 seconds

#### Mode

Global Configuration