# ip dhcp-capture

#### Syntax

ip dhcp-capture { all | receive | transmit } [ priority { low | high } ]

no ip dhcp-capture { all | receive | transmit }

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Configures the E Series router to capture and log DHCP packet information for an interface. By default, DHCP packet information is not captured. The no version restores the default behavior.

#### Options

- all—Captures received and transmitted packets
- receive—Captures received packets
- transmit—Captures transmitted packets
- low—Captured packets arrive with low priority; the default priority
- high—Captured packets arrive with high priority

#### Mode

Interface Configuration