# Monitoring Configured and Operational Summary Status

#### Purpose

Display a summary of the configured and operational status of all L2TP sessions.

#### Action

To display a summary of the configured and operational status of all L2TP sessions:

    host1#show l2tp session summary
    Administrative status  enabled   disabled
                           64        0
    Operational status     up        down   lower-down   not-present
                           64        0      0            0

#### Meaning

Table 92 lists the show l2tp session summary command output fields.

Table 92: show l2tp session summary Output Fields

Field Name | Field Description
--- | ---
Administrative status: | Administrative status of the session: enabled—No restrictions on the creation of sessions disabled—Router disabled these sessions
Operational status: | Operational status of the session: up—Session is available down—Session is unavailable lower-down—Session is unavailable because the tunnel supporting it is inaccessible not-present—Session is unavailable because the hardware (such as a line module) supporting it is inaccessible

#### Related Documentation

- show l2tp session summary