Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# pvc

#### Syntax

To create a control PVC from Interface Configuration mode:

pvc vcd vpi/vci ilmi

no pvc vcd

To create a data PVC from Subinterface Configuration mode and access ATM VC Configuration mode:

pvc vcd vpi/vci

no pvc vcd

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

From Interface Configuration mode, creates a control PVC that supports ILMI services. To create a control PVC, you must specify the VCD, VPI, VCI, and the ilmi encapsulation type. The no version removes the specified control PVC from the router.

From Subinterface Configuration mode, creates a data PVC and accesses ATM VC Configuration mode, from which you can configure and modify individual PVC attributes one at a time. To create a data PVC, you must specify the VCD, VPI, and VCI. The no version removes the specified data PVC from the router.

#### Options

- vcd—Virtual circuit descriptor that is an identifier for the VC in other commands; number, in the range 1–2147483647
- vpi—Virtual path identifier for this PVC. The numeric range depends on the module capabilities and current configuration.
- vci—Virtual circuit identifier for this PVC. The numeric range depends on the module capabilities and current configuration. For control PVCs, the recommended VCI value is 16 for ilmi encapsulation and 5 for qsaal encapsulation. The VCI value cannot be 0.
- ilmi—Configures Integrated Local Management Interface encapsulation for a control PVC

#### Mode

Interface Configuration, Subinterface Configuration

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out