# path ds3 t1 description

#### Syntax

[ no ] path pathChannel ds3 ds3Channel t1 t1Channel [ /subchannel ] description name

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Assigns a text description or an alias to a T1 channel group or subchannel on a DS3 signal. This command applies to a T1 channel group or subchannel on a DS3 over channelized SONET/SDH interface. Use the show controllers sonet command to display the text description. The no version removes the description or alias.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path
- ds3Channel—Number, in the range 1–3, that identifies the DS3 channel
- t1Channel—One or more individual T1 channels, ranges of T1 channels, or combination of individual channels and ranges, in the range 1–28 (no spaces); for example, 3,7-15,19-13,27
- subchannel—Fractional T1 interface in the range 1–24
- name—Text string or alias of up to 80 characters for the T1 channel group or subchannel on a T3 over channelized SONET/SDH interface

#### Mode

Controller Configuration