# redundancy force-switchover

#### Syntax

redundancy force-switchover { slotNumber | srp }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Forces the router to switch from the primary line module in the specified slot or the primary SRP module to the spare line module or SRP module. This command overrides the redundancy lockout command. With the srp option, the command is equivalent to the srp switch command. There is no no version.

| Note: This command replaces the redundancy force-failover command, which has been deprecated.

#### Options

- slotNumber—Number of the slot in which the primary line module resides
- srp—Indicates that the router should switch from the active to the standby SRP module

#### Mode

Privileged Exec