# mroute port admission-bandwidth-limit

#### Syntax

mroute port portNumber admission-bandwidth-limit limitValue
[ priority-bandwidth-limit priorityBandwidthValue ] [ hysteresis hysteresisValue ]

no mroute port portNumber admission-bandwidth-limit

#### Release Information

Command introduced in JunosE Release 7.1.0.
hysteresis and priority-bandwidth limit keywords and hysteresisValue and priorityBandwidthValue variables added in JunosE Release 8.2.0.

#### Description

Configures a limit on the admission bandwidth of outgoing interfaces (OIFs) containing IPv4 or IPv6 mroutes, across different virtual routers, on a port. The no version removes any OIF admission bandwidth limits.

#### Options

- portNumber—Port number in the form slot/port.
- limitValue—Limit on the admission bandwidth (in bits per second) of outgoing interfaces containing IPv4 or IPv6 mroutes, across different virtual routers, on a port. The default is no limit.
- priorityBandwidthValue— Minimum value of admitted priority bandwidth in bps. The default is no limit.
- hysteresisValue—Minimum priority bandwidth limit before the system evaluates mroutes and admits any blocked OIFs; in the range 0-100 percent.

#### Mode

Global Configuration