# baseline ipv6 tcp

#### Syntax

baseline ipv6 tcp [ vrf vrfName ] [ localAddress localPort remoteAddress remotePort ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
ip keyword removed and ipv6 keyword added in JunosE Release 7.2.0.

#### Description

Sets a statistics baseline for only IPv6 TCP statistics. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters
- localAddress—Local IPv6 address on the router
- localPort—Local TCP port number on the router
- remoteAddress—IPv6 address of remote router
- remotePort—TCP port number on remote router

#### Mode

Privileged Exec