Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Per-Packet Queuing on the SAR Scheduler Overview
- Guidelines for Configuring QoS over ATM
- interface atm
- qos-mode-port
- qos-profile

# Configuring Low-Latency Mode for Per-Port Queuing on ATM Interfaces

In low-latency mode, the SAR scheduler backpressures the HRR scheduler per physical port; each physical port buffers only a few kilobytes.

When you configure low-latency mode:

- VC backpressure is disabled.
- Port backpressure is enabled as aggressive.
- SAR scheduler performs minimal buffering.
- HRR scheduler is dominant.

This procedure creates the low-latency mode configuration shown in Figure 1.

Figure 1: Low-Latency Mode

To configure low-latency mode with a strict-priority queue and a best-effort queue:

1. Configure the traffic class.
   host1(config)#traffic-class strict host1(config-traffic-class)#exit
2. Set the traffic class in the traffic-class group.
   host1(config)#traffic-class-group strict host1(config-traffic-class-group)#traffic-class strict host1(config-traffic-class-group)#exit
3. Define the scheduler profile for the traffic-class group.
   host1(config)#scheduler-profile strict host1(config-scheduler-profile)#strict-priority host1(config-scheduler-profile)#exit
4. Configure the QoS profile with two ATM VC queues.
   host1(config)#qos-profile low-latency-q-p host1(config-qos-profile)#atm-vc node host1(config-qos-profile)#atm-vc queue traffic-class best-effort host1(config-qos-profile)#atm group strict scheduler-profile strict host1(config-qos-profile)#atm-vc queue traffic-class strict host1(config-qos-profile)#exit
5. From the desired port, set the QoS port mode to low latency.
   host1(config)#interface atm 2/0 host1(config-if)#qos-mode-port low-latency host1(config-if)#qos-profile low-latency-q-p

   | Tip: For ATM interfaces on ERX7xx models, ERX14xx models, and the ERX310 router, you must specify port 0.

   The qos-mode-port command:

   - Excludes non-UBR ATM QoS services on any VC on the ATM module; for example, PCR, nrtVBR, and CBR
   - Cannot be used if shaping is currently configured on the SAR scheduler
   - Cannot be used with ATM VP tunnels with nonzero rates; however, can be used with tunnels with rates of zero (shapeless tunnels).

## Related Documentation

- Per-Packet Queuing on the SAR Scheduler Overview
- Guidelines for Configuring QoS over ATM
- interface atm
- qos-mode-port
- qos-profile

#### Published: 2011-03-17

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out