# ip igmp version

#### Syntax

ip igmp version { 3 | 2 | 1 | passive }

no ip igmp version

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the IGMP version for the interface. The no version restores the default value, IGMPv2.

#### Options

- 3—Specifies IGMP version 3
- 2—Specifies IGMP version 2
- 1—Specifies IGMP version 1
- passive—Configures a mapped OIF as a passive interface with only multicast-data-forwarding capability

#### Mode

Interface Configuration, Profile Configuration