# pppoe service-name-table

#### Syntax

pppoe service-name-table tableName

no pppoe service-name-table

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

From Interface Configuration or Subinterface Configuration mode, assigns a PPPoE service name table to a PPPoE major interface for use by a static ATM or Ethernet interface. The no version removes the PPPoE service name table assignment.

From Profile Configuration mode, assigns a PPPoE service name table to a profile for use by the dynamic PPPoE interface column associated with the profile. The no version removes the PPPoE service name table assignment.

#### Options

- tableName—Name of the PPPoE service name table; string of up to 31 alphanumeric characters

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration